N902LA 5/19/2022 Tach 2031.5 Installed complete muffler system per manufacturer’s service manual. 
Kenny Maggart 813-404-4771 reinforced the muffler intakes. 
Kenny Maggart thinks the exhaust pipes were heating and cooling creating a bellowing affect on the muffler which caused the intakes to fail. 
Kenny Maggart drilled holes in the bolts that hold the exhaust pipes to the muffler for a cotter key.
Front Right exhaust pipe E6 18-31 01 was installed new.
Keith Carver A/P reviewed the installation of the complete exhaust system
John ? A/P working under Keith Carver did the installation. Exhaust pipes and muffler was mount, then the exhaust pipes were tightened first, then the muffler tightened to the engine. Brackets securing the exhaust pipes to muffler are hand tight to allow exhaust pipes to slip inside the intake holes. 

